Hello.

This is the first rom I have completely modified from stock.  I personally made the boot.img, kernels, and fixed up the system.  I hope it works well for you all.  Up to version 1.5 now.  Good luck and enjoy!


You can just use standard options, I recommend erasing IDB(nand) before flashing. 

Kernel jjhkernel-v3.2-720p is the default.  It has interactive cpu scheduler and ram clocked at 800Mhz.  Vsync-fix applied in both kernels, discovered by phjanderson.  This kernel in this rom scores around 17000+ in Antutu benchmark.

Kernel jjhkernel-v3.2-1080p is also available in the ROM folder, same config as the 720 one but it's 1080.  Just choose it in the flash tool as well as the 1080 boot.

Both of these default kernels sould be good and stable, not generating too much heat.


I am always working on new kernels also.

Warning:  With my kernel the blue light on your stick will not light up when plugged in from a cold boot.  We'll get that figured out eventually.

Also, If you feel a need to install it I have included cwm-recovery to flash after you have successfully installed and booted the rom.  

To install cwm with the flash tool, uncheck all boxes except for recovery, and redirect it to the ROM\cwm-recovery.img file.  Do not erase IDB(nand) before installing cwm, just flash.

As always, flash at your own risk!


jjh


p.s.  Thank you to Finless, Leolas, phjanderson, thesawolf, and anyone else I'm forgetting.